{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C / RXS-K"]
[]
[]
[]
[]
["","","","","FFQ35C2VEB / RXS35K2V1B","FFQ50C2VEB / RXS50K2V1B"]
["Cooling capacity","Nom.","","kW","3.40","5.00"]
["Space cooling","SEER","","","5.60","5.70"]
["","Annual energy consumption","","kWh/a","212","307"]
["","Capacity","Pdesign","kW","3.40","5.00"]
["","Energy efficiency class","","","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.45","3.84"]
["","SCOP/A","","","4.09","4.10"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,182","1,311"]
["Nominal efficiency","EER","","","3.70","3.21"]
["","Annual energy consumption","","kWh","460","780"]
["","COP","","","3.41","3.49"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","4.20","5.80"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]