{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C / RXS-L"]
[]
[]
[]
[]
["","","","","FFQ25C2VEB / RXS25L2V1B","FFQ35C2VEB / RXS35L2V1B","FFQ50C2VEB / RXS50L2V1B","FFQ60C2VEB / RXS60L2V1B"]
["Cooling capacity","Min.","","kW","1.4","1.4","1.7","1.7"]
["","Max.","","kW","4.0","4.0","5.3","6.5"]
["","Nom.","","kW","2.50","3.4","5.0","5.7"]
["Space cooling","SEER","","","6.11","6.32","5.93","5.71"]
["","Annual energy consumption","","kWh/a","143","188","295","349"]
["","Capacity","Pdesign","kW","2.50","3.40","5.00","5.70"]
["","Energy efficiency class","","","A++","A++","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.31","3.10","3.84","3.96"]
["","SCOP/A","","","4.24","4.10","3.90","4.04"]
["","Energy efficiency class","","","A+","A+","A","A+"]
["","Annual energy consumption","","kWh/a","763","1,059","1,378","1,373"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","Annual energy consumption","","kWh","280","460","780","945"]
["","EER","","","4.46","3.70","3.21","3.02"]
["","COP","","","3.90","3.50","3.49","3.41"]
["","Energy labeling Directive","Cooling","","A","A","A","B"]
["","","Heating","","A","B","B","B"]
["Heating capacity","Nom.","","kW","3.20","4.20","5.8","7.0"]
["","Min.","","kW","1.3","1.3","1.7","1.7"]
["","Max.","","kW","5.1","5.1","6.0","8.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]