{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":14,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQG71L8Y1B","FFQ35C2VEB / FFQ35C2VEB / RZQG71L8Y1B","FFQ50C2VEB / FFQ50C2VEB / RZQG71L8Y1B","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQG100L8Y1B","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQG100L8Y1B","FFQ50C2VEB / FFQ50C2VEB / FFQ50C2VEB / RZQG100L8Y1B","FFQ50C2VEB / FFQ50C2VEB / RZQG100L8Y1B","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQG125L8Y1B","FFQ50C2VEB / FFQ50C2VEB / FFQ50C2VEB / RZQG125L8Y1B","FFQ60C2VEB / FFQ60C2VEB / RZQG125L8Y1B"]
["Space cooling","SEER","","","5.10","5.1","5.10","5.10","5.1","5.10","5.1","5.10","5.10","5.1"]
["","Annual energy consumption","","kWh/a","467","467","467","652","652","652","652","824","824","824"]
["","Capacity","Pdesign","kW","6.80","6.8","6.80","9.50","9.5","9.50","9.5","12.00","12.00","12"]
["","Energy efficiency class","","","B","B","B","B","B","B","B","B","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","6","6.00","11.30","11.3","11.30","11.3","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","3.8","3.80","3.80","3.8","3.80","3.8","3.80","3.80","3.8"]
["","Energy efficiency class","","","A","A","A","A","A","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","2,211","2,211","2,211","4,164","4,164","4,164","4,164","4,683","4,683","4,683"]
["Notes","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]