{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQSG100L8Y1B","FFQ50C2VEB / FFQ50C2VEB / RZQSG100L8Y1B","FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / FFQ35C2VEB / RZQSG125L8Y1B","FFQ50C2VEB / FFQ50C2VEB / FFQ50C2VEB / RZQSG125L8Y1B","FFQ60C2VEB / FFQ60C2VEB / RZQSG125L8Y1B"]
["Space cooling","SEER","","","5.1","5.1","4.8","4.8","4.8"]
["","Annual energy consumption","","kWh/a","652","652","875","875","875"]
["","Capacity","Pdesign","kW","9.5","9.5","12","12","12"]
["","Energy efficiency class","","","B","B","B","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","3.8","3.8","3.8","3.8","3.8"]
["","Energy efficiency class","","","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","2,800","2,800","2,800","2,800","2,800"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]