{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":8,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C"]
[]
[]
[]
[]
["","","","","FFQ25C2VEB","FFQ35C2VEB","FFQ50C2VEB","FFQ60C2VEB"]
["Sound pressure level","Heating","High","dBA","31","34","39","43"]
["","","Nom.","dBA","28.5","30.5","34","40"]
["","","Low","dBA","25","25","27","32"]
["","Cooling","Low","dBA","25","25","27","32"]
["","","High","dBA","31","34","39","43"]
["","","Nom.","dBA","28.5","30.5","34","40"]
["Standard Accessories","Operation manual","","","1","1","1","1"]
["","Installation manual","","","1","1","1","1"]
["","Drain hose","","","1","1","1","1"]
["","Metal clamp for drain hose","","","1","1","1","1"]
["","Washer for hanger bracket","","","8","8","8","8"]
["","Screws","","","4","4","4","4"]
["","Paper pattern for installation","","","1","1","1","1"]
["","Insulation for fitting","","","2","2","2","2"]
["","Sealing pad","","","4","4","4","4"]
["","Clamps","","","7","7","7","7"]
["Control systems","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7F530W (white panel), BRC7F530S (grey panel), BRC7EB530W (standard panel)","BRC7F530W (white panel), BRC7F530S (grey panel), BRC7EB530W (standard panel)","BRC7F530W (white panel), BRC7F530S (grey panel), BRC7EB530W (standard panel)","BRC7F530W (white panel), BRC7F530S (grey panel), BRC7EB530W (standard panel)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","dBA","48","51","56","60"]
["Dimensions","Unit","Width","mm","575","575","575","575"]
["","","Depth","mm","575","575","575","575"]
["","","Height","mm","260","260","260","260"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","16","16","17.5","17.5"]
["Decoration panel 2","Weight","","kg","2.8","2.8","2.8","2.8"]
["","Model","","","BYFQ60CS (grey panel)","BYFQ60CS (grey panel)","BYFQ60CS (grey panel)","BYFQ60CS (grey panel)"]
["","Dimensions","Depth","mm","620","620","620","620"]
["","","Width","mm","620","620","620","620"]
["","","Height","mm","46","46","46","46"]
["","Colour","","","White (N9.5) + Silver","White (N9.5) + Silver","White (N9.5) + Silver","White (N9.5) + Silver"]
["Decoration panel 3","Dimensions","Depth","mm","700","700","700","700"]
["","","Height","mm","55","55","55","55"]
["","","Width","mm","700","700","700","700"]
["","Colour","","","White (RAL9010)","White (RAL9010)","White (RAL9010)","White (RAL9010)"]
["","Model","","","BYFQ60B3W1 (standard panel)","BYFQ60B3W1 (standard panel)","BYFQ60B3W1 (standard panel)","BYFQ60B3W1 (standard panel)"]
["","Weight","","kg","2.7","2.7","2.7","2.7"]
["Decoration panel","Weight","","kg","2.8","2.8","2.8","2.8"]
["","Model","","","BYFQ60CW (white panel)","BYFQ60CW (white panel)","BYFQ60CW (white panel)","BYFQ60CW (white panel)"]
["","Dimensions","Height","mm","46","46","46","46"]
["","","Depth","mm","620","620","620","620"]
["","","Width","mm","620","620","620","620"]
["","Colour","","","White (N9.5)","White (N9.5)","White (N9.5)","White (N9.5)"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Dimensions do not include control box","(1) - Dimensions do not include control box","(1) - Dimensions do not include control box","(1) - Dimensions do not include control box"]
["","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]