{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RZAG71M7V1B","FHA35AVEB / FHA35AVEB / RZAG71M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG71M7V1B","FHA50AVEB / FHA50AVEB / RZAG71M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG100M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG100M7V1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZAG100M7V1B","FHA50AVEB / FHA50AVEB / RZAG100M7V1B","FHA71AVEB / FHA71AVEB / RZAG100M7V1B"]
["Cooling capacity","Nom.","","kW","","","","","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Space cooling","Annual energy consumption","","kWh/a","","","","","327","316","368","386","352"]
["","Capacity","Pdesign","kW","","","","","9.50","9.50","9.50","9.50","9.50"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","7.80","7.80","7.80","7.80","7.80"]
["","Annual energy consumption","","kWh/a","","","","","2,256","2,252","2,309","2,405","2,359"]
["Heating capacity","Nom.","","kW","","","","","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Outdoor unit","","","","","RZAG71M7V1B","RZAG71M7V1B","RZAG71M7V1B"]
["Cooling capacity","Nom.","","kW","","6.80 (1)","6.80 (1)","6.80 (1)"]
["Heating capacity","Nom.","","kW","","7.50 (2)","7.50 (2)","7.50 (2)"]
["Space cooling","Energy efficiency class","","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","","6.80","6.80","6.80"]
["","SEER","","","","7.80","7.58","6.55"]
["","Annual energy consumption","","kWh/a","","305","314","363"]
["Space heating (Average climate)","Energy efficiency class","","","","A+","A+","A+"]
["","Capacity","Pdesign","kW","","4.70","4.70","4.70"]
["","SCOP/A","","","","4.43","4.33","4.32"]
["","Annual energy consumption","","kWh/a","","1485","1520","1523"]
["Notes","","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Space cooling","SEER","","","","","","","10.2","10.5","9.04","8.62","9.44"]
["","Energy efficiency class","","","","","","","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","SCOP/A","","","","","","","4.84","4.85","4.73","4.54","4.63"]
["","Energy efficiency class","","","","","","","A++","A++","A++","A+","A++"]