{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B / REQ-BW1"]
[]
[]
[]
[]
["","","","","FHQ71BVV1B / REQ71B8W1B","FHQ100BVV1B / REQ100B8W1B","FHQ125BVV1B / REQ125B8W1B"]
["Cooling capacity","Nom.","","kW","7.10 (3)","9.80 (3)","12.20 (3)"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","15.9"]
["","Drain","OD","mm","26","26","26"]
["Nominal efficiency","EER","","","2.68","2.66","2.71"]
["","Annual energy consumption","","kWh","1,325","1,840","2,255"]
["","COP","","","2.86","2.79","2.81"]
["","Energy labeling Directive","Cooling","","D","D","D"]
["","","Heating","","D","E","D"]
["Heating capacity","Nom.","","kW","8.00 (4)","11.20 (4)","14.50 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]