{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":12,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8"]
[]
[]
[]
[]
["","","","","FHQ35BVV1B","FHQ35BWV1B","FHQ50BWV1B","FHQ60BVV1B","FHQ60BWV1B","FHQ71BVV1B","FHQ100BVV1B","FHQ125BVV1B"]
["Sound pressure level","Heating","High","dBA","37","37","38","39","39","39","42","44"]
["","","Low","dBA","32","32","33","33","33","35","37","39"]
["","Cooling","Low","dBA","32","32","33","33","33","35","37","39"]
["","","High","dBA","37","37","38","39","39","39","42","44"]
["Standard Accessories","Installation and operation manual","","","1","","","1","","1","1","1"]
["","Paper pattern for installation","","","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Sealing pad","","","Sealing pad","","","Sealing pad","","Sealing pad","Sealing pad","Sealing pad"]
["","Clamps","","","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gas","OD","mm","9.52","9.5","12.7","12.70","12.7","15.90","15.90","15.9"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Power input","Cooling","Nom.","kW","","0.111","0.111","","0.115"]
["","Heating","Nom.","kW","","0.111","0.111","","0.115"]
["Sound power level","Cooling","","dBA","53","53","54","55","55","55","58","60"]
["","Heating","","dBA","53","53","54","55","55","55","58","60"]
["Dimensions","Unit","Width","mm","960","960","960","1,160","1,160","1,160","1,400","1,590"]
["","","Depth","mm","680","680","680","680","680","680","680","680"]
["","","Height","mm","195","195","195","195","195","195","195","195"]
["Casing","Colour","","","White","White","White","White","White","White","White","White"]
["Weight","Unit","","kg","24","24","25","27","27","27","32","35"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Operation manual","","","","Operation manual","Operation manual","","Operation manual"]
["","Installation manual","","","","Installation manual","Installation manual","","Installation manual"]
["","Sealing pads","","","","Sealing pads","Sealing pads","","Sealing pads"]