{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQG-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FHQG71CVEB / RZQSG71L2V1B","FHQG100CVEB / RZQSG100L7V1B (Preliminary)","FHQG100CVEB / RZQSG100L7Y1B","FHQG125CVEB / RZQSG125L7Y1B","FHQG140CVEB / RZQSG140L7V1B","FHQG125CVEB / RZQSG125L7V1B","FHQG140CVEB / RZQSG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","9.5 (3)","12.0 (3)","13.4 (3)","","13.4 (3)"]
["Nominal efficiency","Annual energy consumption","","kWh","","","1,480","2,075","2,225","","2,225"]
["Heating capacity","Nom.","","kW","","","10.8 (4)","13.5 (4)","15.5 (4)","","15.5 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - P design (@ -10°C)","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["Cooling capacity","Nom.","","kW","6.8 (3)","","","","","12.0 (3)"]
["Heating capacity","Nom.","","kW","7.5 (4)","","","","","13.5 (4)"]
["Nominal efficiency","EER","","","3.46","","","","","2.89"]
["","COP","","","4.00","","","","","3.62"]
["","Annual energy consumption","","kWh","983","","","","","2075"]
["","Energy labeling Directive","Cooling","","A","","","","","C"]
["","","Heating","","A","","","","","A"]
["Space cooling","SEER","","","5.11","","","","","4.61 (6)"]
["Space heating (Average climate)","SCOP/A","","","3.81","","","","","3.81 (6)"]
["Notes","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(5) - Related to 3D076919","","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825"]
["Space cooling","SEER","","","","","5.11 (6)","4.61 (6)"]
["Space heating (Average climate)","SCOP/A","","","","","3.80 (6)","3.81 (6)"]
["Nominal efficiency","EER","","","","","3.21","2.89","3.01","","3.01"]
["","COP","","","","","3.61","3.62","3.41","","3.41"]
["","Energy labeling Directive","Cooling","","","","A","C","B","","B"]
["","","Heating","","","","A","A","B","","B"]
["Notes","","","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]