{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLKS-B"]
[]
[]
[]
[]
["","","","","FLKS25BAVMB","FLKS35BAVMB","FLKS50BAVMB","FLKS60BAVMB"]
["Sound pressure level","Cooling","Silent operation","dBA","28.0","29.0","36.0","39.0"]
["","","Low","dBA","31.0","32.0","39.0","41.0"]
["","","High","dBA","37.0","38.0","47.0","48.0"]
["","","Nom.","dBA","34.0","35.0","43.0","45.0"]
["Standard Accessories","Installation and operation manual","","","1","1","1","1"]
["","Infrared remote control","","","1","1","1","1"]
["","Batteries","","","2","2","2","2"]
["","Remote control holder","","","1","1","1","1"]
["","Air purification filter","","","1","1","1","1"]
["","Heat insulation tube (refrigerant pipe)","","","1","1","2","2"]
["","Mounting plate","","","1","1","1","1"]
["","Side cover","","","2","","2","2"]
["","Binding band","","","4","4","4","4"]
["","Photocatalytic deodorizing filter","","","1","1","1","1"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7","12.7"]
["","Drain","","","18","18","18","18"]
["Sound power level","Cooling","","dBA","53.0","54.0","63.0","64.0"]
["Dimensions","Unit","Width","mm","1,050","1,050","1,050","1,050"]
["","","Depth","mm","200","200","200","200"]
["","","Height","mm","490","490","490","490"]
["Casing","Colour","","","Almond white","Almond white","Almond white","Almond white"]
["Weight","Unit","","kg","16.0","16.0","17.0","17.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","VM","VM","VM","VM"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220-230","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room."]
["","","","","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]
["Standard Accessories","Quantity","","","","2"]
["","Extension auxiliary pipe","","","","","2","2"]