{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B / RXS-G"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB / RXS25G2V1B","FLXS35BAVMB / RXS35G2V1B","FLXS50BAVMB / RXS50G2V1B"]
["Cooling capacity","Min.","","kW","1.2","1.2","0.9"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.5 (1)","3.5 (1)","4.9 (1)"]
["Nominal efficiency","EER","","","3.85","3.10","2.85"]
["","Annual energy consumption","","kWh","325","565","860"]
["","COP","","","3.47","3.25","3.35"]
["","Energy labeling Directive","Cooling","","A","B","C"]
["","","Heating","","B","C","C"]
["Heating capacity","Nom.","","kW","3.4 (2)","4.0 (2)","6.1 (2)"]
["","Min.","","kW","1.2","1.2","0.9"]
["","Max.","","kW","4.5","5.0","7.5"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]