{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B / RXS-J"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB / RXS25J2V1B","FLXS35BAVMB / RXS35J2V1B","FLXS50BAVMB / RXS50J2V1B"]
["Cooling capacity","Min.","","kW","1.2","1.2","0.9"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.5 (3)","3.5 (3)","4.9 (3)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","18.0","18.0","18.0"]
["Nominal efficiency","EER","","","3.85","3.10","2.85"]
["","Annual energy consumption","","kWh","325","565","860"]
["","COP","","","3.47","3.25","3.35"]
["","Energy labeling Directive","Cooling","","A","B","C"]
["","","Heating","","B","C","C"]
["Heating capacity","Nom.","","kW","3.4 (4)","4.0 (4)","6.1 (4)"]
["","Min.","","kW","1.2","1.4","0.9"]
["","Max.","","kW","4.5","5.0","7.5"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - 220V","(5) - 220V","(5) - 220V"]
["","","","","(6) - 230V","(6) - 230V","(6) - 230V"]
["","","","","(7) - 240V","(7) - 240V","(7) - 240V"]
["","","","","(8) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(8) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(8) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]