{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB / RXS25L2V1B","FLXS50BAVMB / RXS50L2V1B"]
["Cooling capacity","Min.","","kW","1.2","0.9"]
["","Max.","","kW","3.0","5.3"]
["","Nom.","","kW","2.5","4.9"]
["Space cooling","SEER","","","5.19","5.25"]
["","Annual energy consumption","","kWh/a","169","326"]
["","Capacity","Pdesign","kW","2.50","4.90"]
["","Energy efficiency class","","","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.50","4.20"]
["","SCOP/A","","","3.80","3.80"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","921","1,546"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","12.7"]
["","Drain","OD","mm","18.0","20"]
["Nominal efficiency","Annual energy consumption","","kWh","325","860"]
["","EER","","","3.85","2.85"]
["","COP","","","3.54","3.35"]
["","Energy labeling Directive","Cooling","","A","C"]
["","","Heating","","B","C"]
["Heating capacity","Nom.","","kW","3.4","6.1"]
["","Min.","","kW","1.2","0.9"]
["","Max.","","kW","4.5","7.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]