{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FNA35A2VEB / FNA35A2VEB / RZQG71L8Y1B","FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / RZQG100L8Y1B","FNA50A2VEB / FNA50A2VEB / RZQG100L8Y1B","FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / RZQG125L8Y1B","FNA50A2VEB / FNA50A2VEB / FNA50A2VEB / RZQG125L8Y1B","FNA60A2VEB / FNA60A2VEB / RZQG125L8Y1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","9.50 (1)","9.50 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["Space cooling","SEER","","","4.80","5.10","5.10","5.10","5.10","5.10"]
["","Annual energy consumption","","kWh/a","496","652","652","824","824","824"]
["","Capacity","Pdesign","kW","6.80","9.50","9.50","12.0","12.0","12.0"]
["","Energy efficiency class","","","B","A","A","A","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","10.7","11.3","11.3","12.7","12.7"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Energy efficiency class","","","A","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","2,211","3,957","4,164","4,164","4,683","4,683"]
["Nominal efficiency","EER","","","3.06 (3)","3.38 (3)","3.78 (3)","3.05 (3)","3.48 (3)","3.20 (3)"]
["","COP","","","2.94 (3)","2.93 (3)","3.65 (3)","3.03 (3)","3.74 (3)","3.21 (3)"]
["","Energy labeling Directive","Cooling","","B","A","A","B","A","B"]
["","","Heating","","D","D","A","D","A","C"]
["Heating capacity","Nom.","","kW","7.50 (2)","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","13.5 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only"]