{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":9,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB","FNA35A2VEB","FNA50A2VEB","FNA60A2VEB"]
["Sound pressure level","Heating","","High","dBA","33","33","36","36"]
["","","","Nom.","dBA","31","31","33","33"]
["","","","Low","dBA","28","28","30","30"]
["","Cooling","","Medium","dBA","31","31","33","33"]
["","","","Low","dBA","28","28","30","30"]
["","","","High","dBA","33","33","36","36"]
["","","","Nom.","dBA","31","31","33","33"]
["Control systems","Wired remote control","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","","dBA","53","53","56","56"]
["Dimensions","Unit","","Width","mm","790","790","1,190","1,190"]
["","","","Depth","mm","200","200","200","200"]
["","","","Height","mm","620, 720 (2), 720 (1)","620, 720 (2), 720 (1)","620, 720 (2), 720 (1)","620, 720 (2), 720 (1)"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["","Colour","","","","Unpainted","Unpainted","Unpainted","Unpainted"]
["Weight","Unit","","","kg","23.0","23.0","30.0","30.0"]
["Fan","External static pressure","","High","Pa","48","48","49","49"]
["","","","Nom.","Pa","30","30","40","40"]
["","Air flow rate","Heating","High","m³/min","8.7","8.7","16.0","16.0"]
["","","","Low","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8","8","14.8","14.8"]
["","","Cooling","Low","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8","8","14.8","14.8"]
["","","","High","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Name","","","","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs","(1) - Including installation legs"]
["","","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]