{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AT"]
[]
[]
[]
[]
["","","","","FTXA20A2V1BT","FTXA25A2V1BT","FTXA35A2V1BT","FTXA42A2V1BT","FTXA50A2V1BT"]
["Sound pressure level","Heating","High","dBA","39","40","41","45","46"]
["","","Medium","dBA","32","33","33","37","42"]
["","","Silent operation","dBA","19","19","19","21","24"]
["","","Low","dBA","25","25","25","29","33"]
["","Cooling","Medium","dBA","32","33","33","37","39"]
["","","Silent operation","dBA","19","19","19","21","24"]
["","","Low","dBA","25","25","25","29","31"]
["","","High","dBA","39","40","41","45","46"]
["Standard Accessories","Installation manual","","","1","1","1","1","1"]
["","Operation manual","","","1","1","1","1","1"]
["","Air filter","","","2","2","2","2","2"]
["","Infrared remote control","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","1","1","1","1","1"]
["","Screw bag","","","1","1","1","1","1"]
["","Screw cover","","","1","1","1","1","1"]
["","AAA dry-cell batteries","","","2","2","2","2","2"]
["","General safety precautions","","","1","1","1","1","1"]
["Refrigerant","GWP","","","675.0","675.0","675.0","675.0","675.0"]
["Control systems","Wired remote control","","","BRC073","BRC073","BRC073","BRC073","BRC073"]
["","Infrared remote control","","","ARC466A58","ARC466A58","ARC466A58","ARC466A58","ARC466A58"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.50","9.50","9.50","12.70","12.70"]
["","Drain","","","18","18","18","18","18"]
["Power input","Cooling","Nom.","kW","0.020","0.022","0.023","0.028","0.030"]
["","Heating","Nom.","kW","0.020","0.020","0.022","0.036","0.039"]
["Sound power level","Cooling","","dBA","57","57","60","60","60"]
["Dimensions","Unit","Width","mm","798","798","798","798","798"]
["","","Depth","mm","189","189","189","189","189"]
["","","Height","mm","295","295","295","295","295"]
["Casing","Colour","","","Blackwood","Blackwood","Blackwood","Blackwood","Blackwood"]
["Weight","Unit","","kg","12","12","12","12","12"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240"]