{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-J-S / RXG-K"]
[]
[]
[]
[]
["","","","","FTXG25JV1BS / RXG25K2V1B","FTXG35JV1BS / RXG35K2V1B","FTXG50JV1BS / RXG50K2V1B"]
["Cooling capacity","Min.","","kW","","","1.7"]
["","Max.","","kW","","","5.3"]
["","Nom.","","kW","2.50 (3)","3.50 (3)","5.0 (3)"]
["Piping connections","Liquid","OD","mm","","","6.35"]
["","Gas","OD","mm","","","12.7"]
["","Drain","OD","mm","","","18.0"]
["Nominal efficiency","EER","","","4.46","3.93","3.21"]
["","Annual energy consumption","","kWh","280","445","780"]
["","COP","","","4.36","4.04","3.63"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","3.40 (4)","4.00 (4)","5.8 (4)"]
["","Min.","","kW","","","1.7"]
["","Max.","","kW","","","6.5"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","","(7) - 220V"]
["","","","","","","(8) - 230V"]
["","","","","","","(9) - 240V"]
["","","","","","","(10) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]