{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-J-S"]
[]
[]
[]
[]
["","","","","","FTXG25JV1BS","FTXG35JV1BS","FTXG50JV1BS"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","6.8","7.3","8.5"]
["Sound pressure level","Cooling","","Nom.","dBA","32","34","40"]
["Fan","Air flow rate","Heating","Nom.","m³/min","7.9","8.6","9.8"]
["Sound pressure level","Heating","","Nom.","dBA","34","36","40"]
["Power input","Cooling","","Nom.","kW","0.018","0.026","0.032, 0.032, 0.032"]
["","Heating","","Nom.","kW","0.024","0.032","0.038, 0.038, 0.038"]
["Casing","Colour","","","","Silver","Silver","Silver"]
["Dimensions","Unit","","Height","mm","295","295","295"]
["","","","Width","mm","915","915","915"]
["","","","Depth","mm","155","155","155"]
["Weight","Unit","","","kg","11","11","11"]
["Fan","Air flow rate","Cooling","High","m³/min","8.8","10.1","10.3"]
["","","","Low","m³/min","4.7","4.6","6.7"]
["","","","Silent operation","m³/min","3.8","3.9","5.7"]
["","","Heating","High","m³/min","9.6","10.8","11.4"]
["","","","Low","m³/min","6.2","6.4","8.1"]
["","","","Silent operation","m³/min","5.4","5.6","7.1"]
["Sound power level","Cooling","","","dBA","54","58","60"]
["","Heating","","","dBA","55","58","60"]
["Sound pressure level","Cooling","","High","dBA","38","42","44"]
["","","","Low","dBA","25","26","35"]
["","","","Silent operation","dBA","22","23","32"]
["","Heating","","High","dBA","39","42","44"]
["","","","Low","dBA","28","29","35"]
["","","","Silent operation","dBA","25","26","32"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","12.70"]
["","Drain","","","","18","18","18"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Batteries","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Paper pattern for installation","","","","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2","2"]
["Power supply","Name","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - 240V","(4) - 240V"]