{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":10,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JA / RXG-K"]
[]
[]
[]
[]
["","","","","FTXG25JV1BA / RXG25K2V1B","FTXG25JV1BA / RXG25K3V1B","FTXG35JV1BA / RXG35K2V1B","FTXG35JV1BA / RXG35K3V1B","FTXG50JV1BA / RXG50K2V1B","FTXG50JV1BA / RXG50K3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","3.0","3.0","3.8","3.8","5.3","5.3"]
["","Nom.","","kW","2.5 (3)","2.5 (2)","3.5 (3)","3.5 (2)","5.0 (3)","5.0 (2)"]
["Space cooling","SEER","","","","6.53","","6.51","","5.45"]
["","Annual energy consumption","","kWh/a","","134","","188","","321"]
["","Capacity","Pdesign","kW","","2.50","","3.50","","5.00"]
["","Energy efficiency class","","","","A++","","A++","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","2.80","","3.30","","4.60"]
["","SCOP/A","","","","4.34","","4.23","","3.87"]
["","Energy efficiency class","","","","A+","","A+","","A"]
["","Annual energy consumption","","kWh/a","","903","","1,091","","1,660"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","9.52","9.52","12.7","12.7"]
["","Drain","OD","mm","16 or 18","16 or 18","16 or 18","16 or 18","18.0","18.0"]
["Nominal efficiency","EER","","","4.46","4.46 (1)","3.93","3.93 (1)","3.21","3.21 (1)"]
["","Annual energy consumption","","kWh","280","280","445","445","780","780"]
["","COP","","","4.36","4.36 (1)","4.04","4.04 (1)","3.63","3.63 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.4 (4)","3.4 (3)","4.0 (4)","4.0 (3)","5.8 (4)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","4.5","4.5","5.0","5.0","6.5","6.5"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(5) - SL: The silent fan level of the air flow rate setting","","(5) - SL: The silent fan level of the air flow rate setting","","(5) - SL: The silent fan level of the air flow rate setting"]
["","","","","(6) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","","(6) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","","(6) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","(7) - Operation range in combination with Nexura, FVXG-K: min. 10°CDB ~ max. 46°CDB","","(7) - Operation range in combination with Nexura, FVXG-K: min. 10°CDB ~ max. 46°CDB","","(7) - Operation range in combination with Nexura, FVXG-K: min. 10°CDB ~ max. 46°CDB"]
["","","","","(8) - 220V","","(8) - 220V","","(8) - 220V"]
["","","","","(9) - 230V","","(9) - 230V","","(9) - 230V"]
["","","","","(10) - 240V","","(10) - 240V","","(10) - 240V"]
["","","","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(11) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]