{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JW"]
[]
[]
[]
[]
["","","","","FTXG25JV1BW","FTXG35JV1BW","FTXG50JV1BW"]
["Sound pressure level","Heating","High","dBA","39","42","44"]
["","","Silent operation","dBA","25","26","32"]
["","","Low","dBA","28","29","35"]
["","Cooling","Silent operation","dBA","22","23","32"]
["","","Low","dBA","25","26","35"]
["","","High","dBA","38","42","44"]
["","","Nom.","dBA","34","36","40"]
["","Cooling","Nom.","dBA","32","34","40"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter","","","2","2","2"]
["","Operation manual","","","1","1","1"]
["","Installation manual","","","1","1","1"]
["","Wireless remote control","","","1","1","1"]
["","Batteries","","","2","2","2"]
["","Remote control holder","","","1","1","1"]
["","Indoor unit fixing screws","","","2","2","2"]
["","Mounting plate","","","1","1","1"]
["","Paper pattern for installation","","","2","2"]
["Control systems","Infrared remote control","","","ARC466A1","ARC466A1","ARC466A1"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7"]
["","Drain","","","16 or 18","16 or 18","18"]
["Power input","Cooling","Nom.","kW","0.018 (3), 0.018 (4), 0.018 (5)","0.026 (3), 0.026 (4), 0.026 (5)","0.032 (1), 0.032 (2), 0.032 (3)"]
["","Heating","Nom.","kW","0.024 (3), 0.02 (4), 0.02 (5)","0.032 (3), 0.032 (4), 0.032 (5)","0.038 (1), 0.038 (2), 0.038 (3)"]
["Sound power level","Cooling","","dBA","56","60","60"]
["","Heating","","dBA","57","60","60"]
["Dimensions","Unit","Width","mm","915","915","915"]
["","","Depth","mm","155","155","155"]
["","","Height","mm","295","295","295"]
["Casing","Colour","","","White","White","White"]
["Weight","Unit","","kg","11","11","11"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","V1","V1","V1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - 220V"]
["","","","","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(2) - 230V"]
["","","","","(3) - 220V","(3) - 220V","(3) - 240V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]