{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LS / RXG-L"]
[]
[]
[]
[]
["","","","","FTXG20LV1BS / RXG20L2V1B","FTXG25LV1BS / RXG25L2V1B","FTXG35LV1BS / RXG35L2V1B","FTXG50LV1BS / RXG50L2V1B"]
["Cooling capacity","Min.","","kW","1.3 (2)","1.3 (2)","1.4 (2)","1.7 (2)"]
["","Max.","","kW","2.8 (2)","3.0 (2)","3.8 (2)","5.3 (2)"]
["Space cooling","SEER","","","8.52","8.50","7.00","6.70"]
["","Annual energy consumption","","kWh/a","94","99","175","251"]
["","Capacity","Pdesign","kW","2.30","2.40","3.50","4.80"]
["","Energy efficiency class","","","A+++","A+++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.10","2.70","3.00","4.60"]
["","SCOP/A","","","4.60","4.60","4.60","4.24"]
["","Energy efficiency class","","","A++","A++","A++","A+"]
["","Annual energy consumption","","kWh/a","639","821","913","1,519"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","12.7"]
["","Drain","OD","mm","18","18.0","18.0","18.0"]
["Nominal efficiency","EER","","","4.59 (1)","4.59 (1)","3.97 (1)","3.53 (1)"]
["","Annual energy consumption","","kWh","250.5","261.5","441","680"]
["","COP","","","5.00 (1)","4.42 (1)","4.06 (1)","3.65 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Min.","","kW","1.3 (2)","1.3 (2)","1.4 (2)","1.7 (2)"]
["","Max.","","kW","4.3 (2)","4.5 (2)","5.0 (2)","6.5 (2)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - SL: The silent fan level of the air flow rate setting","(3) - SL: The silent fan level of the air flow rate setting","(3) - SL: The silent fan level of the air flow rate setting","(3) - SL: The silent fan level of the air flow rate setting"]
["","","","","(4) - 220V","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - 230V","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","(6) - 240V","(6) - 240V","(6) - 240V","(6) - 240V"]