{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LS / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BS / RXLG25M2V1B","FTXG35LV1BS / RXLG35M2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.0","4.6"]
["","Nom.","","kW","2.5 (2)","3.5 (2)"]
["Space cooling","SEER","","","7.04","6.67"]
["","Annual energy consumption","","kWh/a","124","184"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.64","4.60"]
["","Energy efficiency class","","","A++","A++"]
["","Annual energy consumption","","kWh/a","755","913"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nominal efficiency","EER","","","3.68 (1)","3.57 (1)"]
["","Annual energy consumption","","kWh","340","490"]
["","COP","","","4.31 (1)","3.89 (1)"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","4.4 (2)","5.1 (2)"]
["","Min.","","kW","1.0 (6)","1.0 (6)"]
["","Max.","","kW","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - For rated minimal heating capacity indoor unit fan set to SL tap","(6) - For rated minimal heating capacity indoor unit fan set to SL tap"]
["","","","","(7) - Maximum heating capacity at -15°C outdoor temperature","(7) - Maximum heating capacity at -15°C outdoor temperature"]