{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":16,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 3MXM-M"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM20M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM25M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM25M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM35M2V1B / 3MXM40M2V1B","FTXM25M2V1B / FTXM25M2V1B / 3MXM40M2V1B","FTXM25M2V1B / FTXM35M2V1B / 3MXM40M2V1B","FTXM35M2V1B / FTXM35M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM25M2V1B / 3MXM40M2V1B","FTXM20M2V1B / FTXM50M2V1B / 3MXM68M2V1B","FTXM25M2V1B / FTXM42M2V1B / 3MXM68M2V1B","FTXM35M2V1B / FTXM35M2V1B / 3MXM68M2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","6.80","6.70","6.80"]
["Space cooling","SEER","","","8.52","8.52","8.52","8.50","8.50","8.51","8.50","8.50","8.51","7.78","7.99","8.02"]
["","Annual energy consumption","","kWh/a","165","165","165","165","165","165","165","165","165","306","294","297"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","4.00","6.80","6.70","6.80"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.80","5.00","4.80","5.00","4.80","4.80","4.80","5.00","5.00","4.50","4.30","4.80"]
["","SCOP/A","","","4.24","4.60","4.27","4.63","4.30","4.34","4.37","4.38","4.62","3.90","3.86","4.00"]
["","Energy efficiency class","","","A+","A++","A+","A++","A+","A+","A+","A+","A++","A","A","A+"]
["","Pdh Heating capacity at -10°","","kW","0.9","0.9","0.9","0.9","0.8","0.9","0.8","0.9","0.9"]
["","Annual energy consumption","","kWh/a","1,582","1,521","1,572","1,512","1,560","1,548","1,537","1,598","1,515","1,612","1,559","1,680"]
["Nominal efficiency","Annual energy consumption","","kWh","420","377","415","374","412","413","410","407","376","794","751","723"]
["","EER","","","4.76","5.30","4.82","5.35","4.86","4.84","4.88","4.92","5.32","4.28","4.46","4.70"]
["","COP","","","4.73","5.39","4.77","5.45","4.79","4.90","4.91","4.95","5.41","3.82","3.95","3.81"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.60","4.60","4.60","4.60","4.60","4.60","4.60","4.60","4.60","8.60","8.30","8.60"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]