{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-F"]
[]
[]
[]
[]
["","","","","FTXS60FV1B","FTXS71FV1B"]
["Sound pressure level","Heating","High","dBA","44","46"]
["","","Silent operation","dBA","32","34"]
["","","Low","dBA","35","37"]
["","Cooling","Silent operation","dBA","33","34"]
["","","Low","dBA","36","37"]
["","","High","dBA","45","46"]
["","","Nom.","dBA","40","42"]
["","Cooling","Nom.","dBA","41","42"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter","","","2","2"]
["","Operation manual","","","1","1"]
["","Installation manual","","","1","1"]
["","Batteries","","","2","2"]
["","Remote control holder","","","1","1"]
["","Mounting plate","","","1","1"]
["","Indoor unit fixing screws","","","2","2"]
["","Wireless remote control","","","1","1"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","12.7","15.9"]
["","Drain","","","18","18"]
["Sound power level","Cooling","","dBA","61","62"]
["","Heating","","dBA","60","62"]
["Dimensions","Unit","Width","mm","1,050","1,050"]
["","","Depth","mm","238","238"]
["","","Height","mm","290","290"]
["Casing","Colour","","","White","White"]
["Weight","Unit","","kg","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Name","","","V1","V1"]
["","Frequency","","Hz","50","50"]
["","Voltage","","V","220-240","220-240"]