{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":11,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-J / RXL-J"]
[]
[]
[]
[]
["","","","","FTXS20J2V1B / RXL20J2V1B","FTXS25J2V1B / RXL25J2V1B","FTXS35J2V1B / RXL35J2V1B","FTXS35J2V1B / RXL35J3V1B","FTXS42J2V1B / RXL42J3V1B","FTXS50J2V1B / RXL50J2V1B","FTXS50J2V1B / RXL50J3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","2.0 (3)","2.5 (3)","3.5 (3)","3.5 (2)","4.2 (2)","5.0 (2)","5.0 (2)"]
["","Max.","","kW","2.8","3.2","4.0","4.0","5.0","5.3","5.3"]
["Heating capacity","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","2.7 (4)","3.3 (4)","4.0 (4)","4.0 (3)","5.4 (3)","5.8 (3)","5.8 (3)"]
["","Max.","","kW","4.3","4.7","5.2","5.2","6.0","6.5","6.5"]
["Nominal efficiency","Annual energy consumption","","kWh","225","268","430","430","605","730","730"]
["","COP","","","4.43","4.65","4.21","4.21 (1)","3.72 (1)","3.79 (1)","3.79 (1)"]
["","EER","","","4.44","4.67","4.07","4.07 (1)","3.47 (1)","3.42 (1)","3.42 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","","","","190","269","","330"]
["","Energy efficiency class","","","","","","A++","A","","A"]
["","Capacity","Pdesign","kW","","","","3.50","4.20","","5.00"]
["","SEER","","","","","","6.43","5.47","","5.30"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","","","1,188","1,453","","1,634"]
["","Capacity","Pdesign","kW","","","","3.60","3.90","","4.60"]
["","Energy efficiency class","","","","","","A+","A","","A"]
["","SCOP/A","","","","","","4.24","3.75","","3.94"]
["Piping connections","Drain","OD","mm","","","","18.0","18.0","18.0","18.0"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - 220V","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - 230V","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","","","","(6) - 240V","(6) - 240V","(6) - 240V","(6) - 240V"]
["","","","","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]