{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-J / RXS-J"]
[]
[]
[]
[]
["","","","","FTXS20J2V1B / RXS20J2V1B","FTXS25J2V1B / RXS25J2V1B","FTXS35J2V1B / RXS35J2V1B","FTXS42J2V1B / RXS42J2V1B","FTXS50J2V1B / RXS50J2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Nom.","","kW","2.0 (3)","2.5 (3)","3.5 (3)","4.2 (3)","5.0 (3)"]
["","Max.","","kW","2.8","3.2","4.0","5.0","5.3"]
["Heating capacity","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Nom.","","kW","2.7 (4)","3.3 (4)","4.0 (4)","5.4 (4)","5.8 (4)"]
["","Max.","","kW","4.3","4.7","5.2","6.0","6.5"]
["Nominal efficiency","Annual energy consumption","","kWh","225","268","430","605","730"]
["","COP","","","4.43","4.65","4.21","3.72","3.79"]
["","EER","","","4.44","4.67","4.07","3.47","3.42"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Piping connections","Drain","OD","mm","18.0","18.0","18.0","18.0","18.0"]
["","Gas","OD","mm","9.52","9.52","9.52","9.52","12.7"]
["","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]