{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":10,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-J"]
[]
[]
[]
[]
["","","","","","FTXS20J2V1B","FTXS25J2V1B","FTXS35J2V1B","FTXS42J2V1B","FTXS50J2V1B"]
["Power input","Cooling","","Nom.","kW","0.018","0.018"]
["","Heating","","Nom.","kW","0.021","0.021"]
["Casing","Colour","","","","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","295","295","295","295","295"]
["","","","Width","mm","800","800","800","800","800"]
["","","","Depth","mm","215","215","215","215","215"]
["Weight","Unit","","","kg","9","9","10","10","10"]
["Fan","Air flow rate","Cooling","High","m³/min","9.4","10.8","11.4","11.3","11.6"]
["","","","Low","m³/min","5.5","5.2","5.8","6.8","7.0"]
["","","","Silent operation","m³/min","4.1","3.7","4.4","5.9","6.0"]
["","","Heating","High","m³/min","9.9","11.9","12.4","12.2","12.1"]
["","","","Low","m³/min","6.6","6.4","6.8","7.3","7.6"]
["","","","Silent operation","m³/min","6.2","5.9","6.0","6.4","6.7"]
["","","","Nom.","m³/min","7.4","7.9","11.4","11.3","10.2"]
["","","Heating","Nom.","m³/min","8.2","9.1","9.5","9.7","9.8"]
["Sound power level","Cooling","","","dBA","54","57","59","59","60"]
["","Heating","","","dBA","54","58","59","61","63"]
["Sound pressure level","Cooling","","High","dBA","38","41","45","45","46"]
["","","","Low","dBA","25","25","29","33","34"]
["","","","Silent operation","dBA","22","22","23","30","31"]
["","Heating","","High","dBA","38","42","45","45","47"]
["","","","Low","dBA","28","28","29","33","34"]
["","","","Silent operation","dBA","25","25","26","30","31"]
["","","","Nom.","dBA","32","33","37","39","40"]
["","Heating","","Nom.","dBA","33","35","39","39","41"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","9.52","9.52","12.7"]
["","Drain","","","","I.D. 14.0/O.D. 18.0","I.D. 14.0/O.D. 18.0","I.D. 14.0/O.D. 18.0","I.D. 14.0/O.D. 18.0","I.D. 14.0/O.D. 18.0"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter","","","","2","2","2","2","2"]
["","Operation manual","","","","2","2","2","2","2"]
["","Installation manual","","","","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1"]
["","Batteries","","","","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]