{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":7,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Sound pressure level","Heating","","High","dBA","43"]
["","","","Medium","dBA","35"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","26"]
["","Cooling","","Medium","dBA","35"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","26"]
["","","","High","dBA","43"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Remote control holder","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","16 (inner diameter of connecting hose)"]
["Power input","Cooling","","Nom.","kW","0.030"]
["","Heating","","Nom.","kW","0.035"]
["Sound power level","Cooling","","","dBA","58"]
["","Heating","","","dBA","58"]
["Dimensions","Unit","","Width","mm","770"]
["","","","Depth","mm","225"]
["","","","Height","mm","285"]
["Casing","Colour","","","","White"]
["Weight","Unit","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Name","","","","V1"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - See separate drawing for electrical data"]
["Power input","Cooling","","Nom.","kW","","0.03"]
["","Heating","","Nom.","kW","","0.035"]
["Casing","Colour","","","","","White"]
["Dimensions","Unit","","Height","mm","","285"]
["","","","Width","mm","","770"]
["","","","Depth","mm","","225"]
["Weight","Unit","","","kg","","9"]
["Fan","Air flow rate","Cooling","High","m³/min","","11.4"]
["","","","Medium","m³/min","","8.2"]
["","","","Low","m³/min","","5.4"]
["","","","Silent operation","m³/min","","4.3"]
["","","Heating","High","m³/min","","10.8"]
["","","","Medium","m³/min","","7.8"]
["","","","Low","m³/min","","5.8"]
["","","","Silent operation","m³/min","","4.9"]
["Sound power level","Cooling","","","dBA","","58"]
["","Heating","","","dBA","","58"]
["Sound pressure level","Cooling","","High","dBA","","43"]
["","","","Medium","dBA","","35"]
["","","","Low","dBA","","26"]
["","","","Silent operation","dBA","","21"]
["","Heating","","High","dBA","","43"]
["","","","Medium","dBA","","35"]
["","","","Low","dBA","","26"]
["","","","Silent operation","dBA","","21"]
["Piping connections","Liquid","","OD","mm","","6.35"]
["","Gas","","OD","mm","","9.5"]
["","Drain","","","","","16 (inner diameter of connecting hose)"]
["Control systems","Infrared remote control","","","","","ARC480A11"]
["","Wired remote control","","","","","BRC944B2, BRC073A1"]
["Power supply","Name","","","","","V1"]
["","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]