{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-B8 / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FUQ71BWV1B / RZQG71L7V1B","FUQ71BWV1B / RZQG71L7Y1B","FUQ100BWV1B / RZQG100L7V1B","FUQ100BWV1B / RZQG100L7Y1B","FUQ125BWV1B / RZQG125L7V1B","FUQ125BWV1B / RZQG125L7Y1B"]
["Cooling capacity","Nom.","","kW","6.8 (3)","6.8 (3)","9.5 (3)","9.5 (3)","12.0 (3)","12.0 (3)"]
["Space cooling","SEER","","","5.25 (6)","5.25 (6)","4.67 (6)","4.67 (6)","4.41 (6)","4.41 (6)"]
["Space heating (Average climate)","SCOP/A","","","3.89 (6)","3.89 (6)","4.02 (6)","4.02 (6)","4.09 (6)","4.09 (6)"]
["Nominal efficiency","EER","","","4.05","4.05","3.86","3.86","3.39","3.39"]
["","Annual energy consumption","","kWh","840","840","1,230","1,230","1,770","1,770"]
["","COP","","","4.08","4.08","3.95","3.95","3.42","3.42"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","B","B"]
["Heating capacity","Nom.","","kW","7.5 (4)","7.5 (4)","10.8 (4)","10.8 (4)","13.5 (4)","13.5 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825","(6) - SEER and SCOP are according to EN 14825"]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]