{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-B"]
[]
[]
[]
[]
["","","","","FVQ71BV1B","FVQ100BV1B","FVQ125BV1B"]
["Sound pressure level","Heating","High","dBA","42","48","50"]
["","","Low","dBA","36","42","44"]
["","Cooling","Low","dBA","36","42","44"]
["","","High","dBA","42","48","50"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual"]
["","Bracket for installation","","","Bracket for installation","Bracket for installation","Bracket for installation"]
["","Through hole protecting rubber","","","Through hole protecting rubber","Through hole protecting rubber","Through hole protecting rubber"]
["","Bush","","","Bush","Bush","Bush"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Control panel patch plate","","","Control panel patch plate","Control panel patch plate","Control panel patch plate"]
["","Remote control lid","","","Remote control lid","Remote control lid","Remote control lid"]
["","Clamps","","","Clamps","Clamps","Clamps"]
["","Screws","","","Screws","Screws","Screws"]
["","Installation pattern","","","Installation pattern","Installation pattern","Installation pattern"]
["Piping connections","Liquid","OD","mm","","","9.52"]
["","Gas","OD","mm","","","15.90"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Sound power level","Cooling","","dBA","54","60","62"]
["","Heating","","dBA","54","60","62"]
["Dimensions","Unit","Width","mm","600","600","600"]
["","","Depth","mm","270","350","350"]
["","","Height","mm","1,850","1,850","1,850"]
["Casing","Colour","","","White","White","White"]
["Weight","Unit","","kg","39","46","47"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]