{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F / RXM-N"]
[]
[]
[]
[]
["","","","","FVXM50FV1B / RXM50N2V1B","FVXM50FV1B9 / RXM50N2V1B"]
["Cooling capacity","Min.","","kW","1.40","1.40"]
["","Max.","","kW","5.60","5.60"]
["","Nom.","","kW","5.00","5.00"]
["Space cooling","SEER","","","6.80","6.80"]
["","Annual energy consumption","","kWh/a","257","257"]
["","Capacity","Pdesign","kW","5.00","5.00"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.20","4.20"]
["","SCOP/A","","","4.00","4.00"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,471","1,471"]
["Nominal efficiency","EER","","","3.23","3.23"]
["","Annual energy consumption","","kWh","773","773"]
["","COP","","","3.63","3.63"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","5.80","5.80"]
["","Min.","","kW","1.40","1.40"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]