{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":11,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F"]
[]
[]
[]
[]
["","","","","","FVXM25FV1B","FVXM25FV1B9","FVXM35FV1B","FVXM35FV1B9","FVXM50FV1B9","FVXM50FV1B"]
["Power input","Cooling","","Nom.","kW","0.015","0.015","0.015","0.015","0.027","0.027"]
["","Heating","","Nom.","kW","0.017","0.017","0.017","0.017","0.034","0.034"]
["Casing","Colour","","","","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","600","600","600","600","600","600"]
["","","","Width","mm","700","700","700","700","700","700"]
["","","","Depth","mm","210","210","210","210","210","210"]
["Weight","Unit","","","kg","14","14","14","14","14","14"]
["Fan","Air flow rate","Cooling","High","m³/min","8.2","8.2","8.5","8.5","10.1","10.1"]
["","","","Medium","m³/min","6.5","6.5","6.7","6.7","8.9","8.9"]
["","","","Low","m³/min","4.8","4.8","4.9","4.9","7.8","7.8"]
["","","","Silent operation","m³/min","4.1","4.1","4.5","4.5","6.6","6.6"]
["","","Heating","High","m³/min","8.8","8.8","9.4","9.4","11.8","11.8"]
["","","","Medium","m³/min","6.9","6.9","7.3","7.3","10.1","10.1"]
["","","","Low","m³/min","5","5","5.2","5.2","8.5","8.5"]
["","","","Silent operation","m³/min","4.4","4.4","4.7","4.7","7.1","7.1"]
["Sound power level","Cooling","","","dBA","52","52","52","52","57","57"]
["","Heating","","","dBA","52","52","52","52","58","58"]
["Sound pressure level","Cooling","","High","dBA","38","38","39","39","44","44"]
["","","","Medium","dBA","32","32","33","33","40","40"]
["","","","Low","dBA","26","26","27","27","36","36"]
["","","","Silent operation","dBA","23","23","24","24","32","32"]
["","Heating","","High","dBA","38","38","39","39","45","45"]
["","","","Medium","dBA","32","32","33","33","40","40"]
["","","","Low","dBA","26","26","27","27","36","36"]
["","","","Silent operation","dBA","23","23","24","24","32","32"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC452A1","ARC452A1","ARC452A1","ARC452A1","ARC452A1","ARC452A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1"]
["","Installation plate","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2"]
["","Drain hose","","","","1","1","1","1","1","1"]
["","Insulation sheet","","","","2","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-230-240","220-230-240","220-230-240","220-230-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V","(1) - 50Hz, 220-230-240V"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]