{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-J"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25J2V1B","FVXS25FV1B / RXL25J3V1B (Preliminary)","FVXS35FV1B / RXL35J2V1B","FVXS35FV1B / RXL35J3V1B","FVXS50FV1B / RXL50J2V1B","FVXS50FV1B / RXL50J3V1B"]
["Cooling capacity","Min.","","kW","1.3","","1.4","1.4","1.4","1.4"]
["","Max.","","kW","3.0","","3.8","3.8","5.6","5.6"]
["","Nom.","","kW","2.5 (3)","","3.5 (3)","3.5 (2)","5.0 (2)","5.0 (2)"]
["Space cooling","SEER","","","","","","4.93","","5.53"]
["","Annual energy consumption","","kWh/a","","","","248","","317"]
["","Capacity","Pdesign","kW","","","","3.50","","5.00"]
["","Energy efficiency class","","","","","","B","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","2.90","","4.80"]
["","SCOP/A","","","","","","3.77","","3.59"]
["","Energy efficiency class","","","","","","A","","A"]
["","Annual energy consumption","","kWh/a","","","","1,077","","1,874"]
["Piping connections","Liquid","OD","mm","6.35","","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","","","","20.0","20.0","20.0"]
["Nominal efficiency","EER","","","4.39","","4.30","3.43 (1)","3.23 (1)","3.23 (1)"]
["","Annual energy consumption","","kWh","285","","407","510","775","775"]
["","COP","","","3.43","","3.69","3.69 (1)","3.63 (1)","3.63 (1)"]
["","Energy labeling Directive","Cooling","","A","","A","A","A","A"]
["","","Heating","","B","","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.4 (4)","","4.5 (4)","4.5 (3)","5.8 (3)","5.8 (3)"]
["","Min.","","kW","1.3","","1.4","1.4","1.4","1.4"]
["","Max.","","kW","4.5","","5.0","5.0","8.1","8.1"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","","","","(6) - 240V","(6) - 240V","(6) - 240V"]
["","","","","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]