{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-M"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25M2V1B","FVXS35FV1B / RXL35M2V1B"]
["Outdoor unit","","","","RXL25M","RXL35M"]
["Cooling capacity","Nom.","","kW","2.50","3.50"]
["Heating capacity","Nom.","","kW","3.50","4.60"]
["","Max.","","kW","3.30 (1), 3.40 (2)","3.70 (1), 3.80 (2)"]
["Piping connections","Gas","OD","mm","9.5","9.5"]
["","Liquid","OD","mm","6.35","6.35"]
["Space cooling","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","2.50","3.50"]
["","SEER","","","5.83","5.95"]
["","Annual energy consumption","","kWh/a","150","206"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","2.60","3.10"]
["","SCOP/A","","","4.45","4.30"]
["","Annual energy consumption","","kWh/a","818","1009"]
["Notes","","","","(1) - Maximum average heating capacity at -15°C","(1) - Maximum average heating capacity at -15°C"]
["","","","","(2) - Maximum peak heating capacity at -15°C","(2) - Maximum peak heating capacity at -15°C"]