{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MKS-E"]
[]
[]
[]
[]
["","","","","","3MKS50E2V1B","4MKS58E2V1B","5MKS90E7V3B"]
["Sound pressure level","Cooling","","Nom.","dBA","46","46","48"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1"]
["","Air direction adjustment plate","","","","1","1"]
["Refrigerant","Charge","","","kg","2.0","2.0","2.95"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","m","15","15","7.5"]
["","","IU - OU","Max.","m","15","15","15"]
["","Additional refrigerant charge","","","kg/m","Chargeless","Chargeless","0.02 (for piping length exceeding 65m)"]
["Sound power level","Cooling","","","dBA","59","59","62"]
["Dimensions","Unit","","Width","mm","936","936","900"]
["","","","Depth","mm","300","300","320"]
["","","","Height","mm","735","735","770"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","49","49","69"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m"]
["Standard Accessories","Reducer assembly","","","","","1","1"]