{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RMXS-EV"]
[]
[]
[]
[]
["","","","","","RMXS112E8V1B","RMXS140E8V1B","RMXS160E8V1B"]
["Sound pressure level","Heating","","Nom.","dBA","53","54","55"]
["","Cooling","","Nom.","dBA","51","52","54"]
["","Night quiet mode","","Level 3","dBA","41.0","41.0","41.0"]
["","","","Level 1","dBA","47","47","47"]
["","","","Level 2","dBA","44.0","44.0","44.0"]
["Standard Accessories","Gas connection pipe","","","","3","3","3"]
["","Installation manual","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain socket","","","","1","1","1"]
["","Drain cap","","","","2","2","2"]
["","Drain receiver","","","","3","3","3"]
["","Insulation","","","","1","1","1"]
["Maximum number of connectable indoor units (BP to be connected)","","","","","6","8","9"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A"]
["Indoor index connection","Min.","","","","55","70","80"]
["","Max.","","","","145.5","182","208"]
["Cooling capacity","Nom.","","","kW","11.2 (1)","14.0 (1)","15.5 (1)"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52"]
["","","","Type","","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","19.1","19.1","19.1"]
["","","","Type","","Braze connection","Braze connection","Braze connection"]
["","Drain","","OD","mm","26x3","26x3","26x3"]
["","","","Type","","Hole","Hole","Hole"]
["","Level difference","IU - IU","Max.","m","15","15","15"]
["","","","OU - IU","m","30","30","30"]
["","","IU - OU","Max.","m","30","30","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual"]
["","Total piping length","System","Actual","m","115","135","145"]
["Sound power level","Cooling","","Nom.","dBA","67","68","70"]
["COP","","","","","3.18","3.07","3.22"]
["Dimensions","Unit","","Width","mm","900","900","900"]
["","","","Depth","mm","320","320","320"]
["","","","Height","mm","1,345","1,345","1,345"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","120","120","120"]
["EER","","","","","3.20","2.75","2.87"]
["Heating capacity","Nom.","","","kW","12.5 (2)","16.0 (2)","17.5 (2)"]
["Power supply","Phase","","","","1N~","1N~","1N~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m; level difference: 0m.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m; level difference: 0m.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m; level difference: 0m."]
["","","","","","(2) - Heating: indoor temp. 20°CDB, outdoor temp. 7°CDB, 6°CWB, equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m / level difference: 0m.","(2) - Heating: indoor temp. 20°CDB, outdoor temp. 7°CDB, 6°CWB, equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m / level difference: 0m.","(2) - Heating: indoor temp. 20°CDB, outdoor temp. 7°CDB, 6°CWB, equivalent piping length: outdoor - BP: 5m / BP - indoor: 3m / level difference: 0m."]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(4) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(4) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(4) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(5) - Sound levels are measured in an anechoic room.","(5) - Sound levels are measured in an anechoic room.","(5) - Sound levels are measured in an anechoic room."]
["","","","","","(6) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(6) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(6) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA"]
["","","","","","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker"]
["","","","","","(11) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(11) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(11) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","(12) - MSC means the maximum current during start up of the compressor","(12) - MSC means the maximum current during start up of the compressor","(12) - MSC means the maximum current during start up of the compressor"]
["","","","","","(13) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(13) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(13) - EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]
["","","","","","(14) - Ssc: Short-circuit power","(14) - Ssc: Short-circuit power","(14) - Ssc: Short-circuit power"]
["","","","","","(15) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(15) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(15) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]