{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RN-E"]
[]
[]
[]
[]
["","","","","","RN50E3V1B","RN60E3V1B"]
["Dimensions","Unit","","Height","mm","735","735"]
["","","","Width","mm","825","825"]
["","","","Depth","mm","300","300"]
["Weight","Unit","","","kg","47","47"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10.0","-10.0"]
["","","","Max.","°CDB","46.0","46.0"]
["Sound pressure level","Cooling","","Nom.","dBA","47","49"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","Charge","","","kg","1.5","1.5"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - IU","Max.","m","20.0","20"]
["Standard Accessories","Installation manual","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]