{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RQ-BW1"]
[]
[]
[]
[]
["","","","","","RQ71B8W1B","RQ71B2W1B","RQ100B8W1B","RQ125B8W1B"]
["Sound pressure level","Cooling","","Nom.","dBA","50.0","50.0","53.0","53.0"]
["Standard Accessories","Declaration of conformity","","","","1","1","1","1"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","5.6","5.6","7.7","7.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","2.70","2.70","3.70","3.70"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","46.0","46.0","46.0","46.0"]
["","","","Min.","°CDB","-5.0","-5.0","-5.0","-5.0"]
["","Heating","Ambient","Max.","°CWB","15.0","15.0","15.0","15.0"]
["","","","Min.","°CWB","-10.0","-10.0","-10.0","-10.0"]
["Piping connections","Piping length","OU - IU","Max.","m","70","70","70","70"]
["","","System","Chargeless","m","30","30","30","30"]
["","","","Equivalent","m","90","90","90","90"]
["","Level difference","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["","","IU - OU","Max.","m","30.0","30.0","30.0","30.0"]
["Sound power level","Cooling","","","dBA","63.0","63.0","66.0","67.0"]
["Dimensions","Unit","","Width","mm","900","900","900","900"]
["","","","Depth","mm","320","320","320","320"]
["","","","Height","mm","770","770","1,170","1,170"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","83","83","101","108"]
["Power supply","Phase","","","","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","400","400","400","400"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]