{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":12,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RR-BW1"]
[]
[]
[]
[]
["","","","","","RR71B7W1B","RR71B8W1B","RR71B2W1B","RR100B7W1B","RR100B8W1B","RR125B7W1B","RR125B8W1B"]
["Sound pressure level","Cooling","","Nom.","dBA","50","50.0","50.0","","","53","53.0"]
["Standard Accessories","Declaration of conformity","","","","1","1","1","1","1","1","1"]
["","Installation manual","","","","1","1","1","1","1","1","1"]
["Refrigerant","Charge","","","kg","2.70","2.70","2.70","","","3.70","3.70"]
["","Type","","","","R-410A","R-410A","R-410A","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","46.0","46.0","46.0","","","46.0","46.0"]
["","","","Min.","°CDB","-15.0","-15.0","-15.0","","","-15.0","-15.0"]
["Piping connections","Piping length","OU - IU","Max.","m","70","70","70","","","70","70"]
["","","System","Chargeless","m","30","30","30","","","30","30"]
["","","","Equivalent","m","90","90","90","","","90","90"]
["","Level difference","IU - IU","Max.","m","0.0","0.5","0.5","","","0.0","0.5"]
["","","IU - OU","Max.","m","30.0","30.0","30.0","","","30.0","30.0"]
["Sound power level","Cooling","","","dBA","63","63.0","63.0","","","67","67.0"]
["Dimensions","Unit","","Width","mm","900","900","900","","","900","900"]
["","","","Depth","mm","320","320","320","","","320","320"]
["","","","Height","mm","770","770","770","","","1,170","1,170"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","81","81","81","","","106","106"]
["Power supply","Phase","","","","3N~","3N~","3N~","","","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","","","50","50"]
["","Voltage","","","V","400","400","400","","","400","400"]
["Notes","","","","","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","","","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(1) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(3) - Sound values are measured in a semi-anechoic room.","(3) - Sound values are measured in a semi-anechoic room.","(3) - Sound values are measured in a semi-anechoic room.","","","(3) - Sound values are measured in a semi-anechoic room.","(3) - Sound values are measured in a semi-anechoic room."]
["","","","","","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit","","","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit","(4) - Heating capacity is only applicable for combination with heat pump outdoor unit"]
["","","","","","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed.","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed.","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed.","","","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed.","(5) - In case of drain piping for the outdoor unit, a drain piping kit (option) is needed."]
["","","","","","(6) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal); level difference: 0m","(6) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(6) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","","","(6) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal); level difference: 0m","(6) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","","","","","(7) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["Dimensions","Unit","","Height","mm","","","","1170","1170"]
["","","","Width","mm","","","","900","900"]
["","","","Depth","mm","","","","320","320"]
["Weight","Unit","","","kg","","","","99","99"]
["Compressor","Type","","","","","","","Hermetically sealed scroll compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","","-15","-15.0"]
["","","","Max.","°CDB","","","","46","46.0"]
["Sound power level","Cooling","","","dBA","","","","66","66.0"]
["Sound pressure level","Cooling","","Nom.","dBA","","","","53","53.0"]
["Refrigerant","Type","","","","","","","R-410A"]
["","Charge","","","kg","","","","3.7","3.70"]
["Piping connections","Piping length","OU - IU","Max.","m","","","","70","70"]
["","","System","Equivalent","m","","","","90","90"]
["","","","Chargeless","m","","","","30","30"]
["","Level difference","IU - OU","Max.","m","","","","30.0","30.0"]
["","","IU - IU","Max.","m","","","","0","0.5"]
["Power supply","Phase","","","","","","","3N~"]
["","Frequency","","","Hz","","","","50","50"]
["","Voltage","","","V","","","","400"]