{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-J"]
[]
[]
[]
[]
["","","","","","RXG25J2V1B","RXG35J2V1B"]
["Sound pressure level","Heating","","High","dBA","","48"]
["","","","Low","dBA","","45"]
["","Cooling","","Low","dBA","","44"]
["","","","High","dBA","","48"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Drain socket","","","","Drain socket","Drain socket"]
["Refrigerant","Charge","","","TCO2Eq","","2.2"]
["","GWP","","","","","2,087.5"]
["","Charge","","","kg","","1.05"]
["","Type","","","","","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","m","","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)"]
["Sound power level","Cooling","","","dBA","","63"]
["Dimensions","Unit","","Width","mm","","765"]
["","","","Depth","mm","","285"]
["","","","Height","mm","","550"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","34"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]
["","","","","","","(4) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","550"]
["","","","Width","mm","765"]
["","","","Depth","mm","285"]
["Weight","Unit","","","kg","34"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Sound pressure level","Cooling","","High","dBA","46"]
["","","","Low","dBA","43"]
["","Heating","","High","dBA","47"]
["","","","Low","dBA","44"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","1.05"]
["","Charge","","","tCO2Eq","2.2"]
["","GWP","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]