{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-G"]
[]
[]
[]
[]
["","","","","","RXS20G2V1B","RXS25G2V1B","RXS35G2V1B","RXS42G2V1B","RXS50G2V1B"]
["Dimensions","Unit","","Height","mm","550","550","550","550","735"]
["","","","Width","mm","765","765","765","765","825"]
["","","","Depth","mm","285","285","285","285","300"]
["Weight","Unit","","","kg","32","34","34","39","48"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","20","20","20","20","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","48","48","48"]
["","","","Low","dBA","43","43","44","44","44"]
["","Heating","","High","dBA","47","47","48","48","48"]
["","","","Low","dBA","44","44","45","45","45"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Charge","","","kg","0.8","1.0","1.2","1.3","1.7"]
["","Charge","","","tCO2Eq","1.7","2.1","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","20","20","20","20","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15.0","15.0","15.0","15.0","20.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]