{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-J"]
[]
[]
[]
[]
["","","","","","RXS20J2V1B","RXS25J2V1B","RXS35J2V1B","RXS42J2V1B","RXS50J2V1B"]
["Sound pressure level","Heating","","High","dBA","47","47","48","48","48"]
["","Cooling","","High","dBA","46","46","48","48","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.7","2.1","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.8","1.0","1.2","1.3","1.7"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","780","780","780","790","670"]
["","","Heating","Super low","rpm","740","740","740","780","670"]
["Piping connections","Level difference","IU - OU","Max.","m","15","15","15","15","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Sound power level","Cooling","","","dBA","61","61","63","63","63"]
["Dimensions","Unit","","Width","mm","765","765","765","765","825"]
["","","","Depth","mm","285","285","285","285","300"]
["","","","Height","mm","550","550","550","550","735"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","32","34","34","39","48"]
["Fan","Air flow rate","Heating","Super low","cfm","1,006","904","904","960","1,522"]
["","","Cooling","Super low","cfm","1,155","1,063","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]