{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-B9W1"]
[]
[]
[]
[]
["","","","","","RZQ100B9W1B","RZQ125B9W1B","RZQ140B9W1B"]
["Sound pressure level","Heating","","Nom.","dBA","51.0","52.0","52.0"]
["","Cooling","","Nom.","dBA","49.0","50.0","50.0"]
["","Night quiet mode","","Level 1","dBA","45.0","45.0","45.0"]
["Standard Accessories","Tie-wraps","","","","2","2","2"]
["","Installation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","9","9","9"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","4.30","4.30","4.30"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Piping connections","Piping length","OU - IU","Max.","m","75","75","75"]
["","","System","Chargeless","m","30","30","30"]
["","","","Equivalent","m","95","95","95"]
["","Level difference","IU - IU","Max.","m","0.5","0.5","0.5"]
["","","IU - OU","Max.","m","30.0","30.0","30.0"]
["","Additional refrigerant charge","","","kg/m","See installation manual 4PW21412-1","See installation manual 4PW21412-1","See installation manual 4PW21412-1"]
["Sound power level","Cooling","","","dBA","65.0","66.0","66.0"]
["Dimensions","Unit","","Width","mm","900","900","900"]
["","","","Depth","mm","320","320","320"]
["","","","Height","mm","1,345","1,345","1,345"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","106","106","106"]
["Power supply","Phase","","","","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","","(2) - Power supply intake for FDQ: outdoor unit + indoor unit","(2) - Power supply intake for FDQ: outdoor unit + indoor unit","(2) - Power supply intake for FDQ: outdoor unit + indoor unit"]
["","","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]