{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","","RZQ71D3V1B","RZQ100D9V1B","RZQ125D9V1B","RZQ140D9V1B"]
["Sound pressure level","Heating","","Nom.","dBA","50","52","53","53"]
["","Cooling","","Nom.","dBA","48","50","51","51"]
["","Night quiet mode","","Level 1","dBA","43","45","45","46"]
["Standard Accessories","Tie-wraps","","","","2","2","2","2"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","5.7","8.2","8.2","8.2"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","2.75","3.95","3.95","3.95"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Piping length","OU - IU","Max.","m","50","75","75","75"]
["","","System","Chargeless","m","30","30","30","30"]
["","","","Equivalent","m","70","95","95","95"]
["","Level difference","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["","","IU - OU","Max.","m","30.0","30.0","30.0","30.0"]
["","Additional refrigerant charge","","","kg/m","See installation manual 4PW48323-1","See installation manual 4PW48323-1","See installation manual 4PW48323-1","See installation manual 4PW48323-1"]
["Sound power level","Cooling","","","dBA","64","65","67","68"]
["Dimensions","Unit","","Width","mm","900","900","900","900"]
["","","","Depth","mm","320","320","320","320"]
["","","","Height","mm","770","1,345","1,345","1,345"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","67","109","109","109"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","","(2) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(2) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(2) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A","(2) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]
["","","","","","(3) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc (=Short-circuit power) value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","","(4) - 230V","(4) - 230V","(4) - 230V","(4) - 230V"]
["","","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases","(5) - Power supply to the FDQ indoor unit is separate","(5) - Contains fluorinated greenhouse gases"]
["","","","","","","","(6) - Contains fluorinated greenhouse gases"]