{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-LV1L"]
[]
[]
[]
[]
["","","","","","RZQG71L9V1L"]
["Sound power level","Cooling","","","dBA","64"]
["Dimensions","Unit","","Height","mm","990"]
["","","","Width","mm","940"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","69.0"]
["Operation range","Cooling","Ambient","Min.","°CDB","-15"]
["","","","Max.","°CDB","50"]
["","Heating","Ambient","Min.","°CWB","-20"]
["","","","Max.","°CWB","16"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","50"]
["","Night quiet mode","","Level 1","dBA","43"]
["Refrigerant","Charge","","","kg","2.9"]
["","Charge","","","tCO2Eq","6.10"]
["","GWP","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","50"]
["","Level difference","IU - OU","Max.","m","30.0"]
["","","IU - IU","Max.","m","0.5"]
["Standard Accessories","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Power supply","Frequency","","","Hz","50"]
["Notes","","","","","(1) - 3 with re-charging"]