{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":9,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQS-DV1"]
[]
[]
[]
[]
["","","","","","RZQS71D7V1B","RZQS100D7V1B","RZQS125D7V1B","RZQS140D7V1B"]
["Sound pressure level","Heating","","Nom.","dBA","51","55","53","54"]
["","Cooling","","Nom.","dBA","49","51","51","52"]
["","Night quiet mode","","Level 1","dBA","47","49","49","50"]
["Standard Accessories","Tie-wraps","","","","2","2","2","2"]
["","Installation manual","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","5.7","7.7","7.7","7.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","2.75","3.7","3.7","3.7"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52","9.52"]
["","Piping length","OU - IU","Max.","m","30","50","50","50"]
["","","System","Chargeless","m","30","30","30","30"]
["","","","Equivalent","m","40","70","70","70"]
["","Gas","","OD","mm","15.9","15.9","15.9","15.9"]
["","Level difference","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["","","IU - OU","Max.","m","15","30","30","30"]
["","Additional refrigerant charge","","","kg/m","See installation manual 4PW49302-1","See installation manual 4PW49302-1","See installation manual 4PW49302-1","See installation manual 4PW49302-1"]
["Sound power level","Cooling","","","dBA","65","67","67","68"]
["Dimensions","Unit","","Width","mm","900","900","900","900"]
["","","","Depth","mm","320","320","320","320"]
["","","","Height","mm","770","1,170","1,170","1,170"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","68","103","103","103"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(1) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(1) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(1) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","","(2) - Ssc: Short-circuit power","(2) - Ssc: Short-circuit power","(2) - Ssc: Short-circuit power","(2) - Ssc: Short-circuit power"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Power supply to the FDQ indoor unit is separate","(4) - Contains fluorinated greenhouse gases"]
["","","","","","","","(5) - Contains fluorinated greenhouse gases"]