{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-C"]
[]
[]
[]
[]
["","","","","ACQ100CV1","ACQ125CV1"]
["Sound pressure level","Heating","High","dBA","44","47"]
["","","Nom.","dBA","41","44"]
["","","Silent operation","dBA","36","41"]
["","","Low","dBA","38","43"]
["","Cooling","Silent operation","dBA","36","41"]
["","","Low","dBA","38","43"]
["","","High","dBA","44","47"]
["","","Nom.","dBA","41","44"]
["Standard Accessories","Installation manual","","","Installation manual","Installation manual"]
["","Operation manual","","","Operation manual","Operation manual"]
["","Screws","","","Screws","Screws"]
["","Washer","","","Washer","Washer"]
["","Wireless remote control","","","Wireless remote control","Wireless remote control"]
["","Cover lock grill","","","Cover lock grill","Cover lock grill"]
["","Battery","","","Battery","Battery"]
["Control systems","Wired remote control","","","ARCWB","ARCWB"]
["Piping connections","Liquid","OD","mm","9.52","9.52"]
["","Gas","OD","mm","15.88","15.88"]
["","Drain","","","19.05","19.05"]
["Power input","Cooling","Nom.","kW","0.094","0.137"]
["","Heating","Nom.","kW","0.094","0.137"]
["Sound power level","Cooling","","dBA","57","60"]
["","Heating","","dBA","56","60"]
["Dimensions","Unit","Width","mm","820","820"]
["","","Depth","mm","820","820"]
["","","Height","mm","300","300"]
["Casing","Material","","","Galvanised steel","Galvanised steel"]
["Weight","Unit","","kg","39","39"]
["Decoration panel","Weight","","kg","4","4"]
["","Dimensions","Height","mm","82","82"]
["","","Depth","mm","990","990"]
["","","Width","mm","990","990"]
["","Colour","","","White","White"]
["Power supply","Phase","","","1~","1~"]
["","Name","","","V1","V1"]
["","Frequency","","Hz","50","50"]
["","Voltage","","V","220-240","220-240"]