{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-B"]
[]
[]
[]
[]
["","","","","FUQ71BVV1B","FUQ100BVV1B","FUQ125BVV1B"]
["Sound pressure level","Heating","High","dBA","40","43.0","44"]
["","","Low","dBA","35","38.0","39"]
["","Cooling","Low","dBA","35","38.0","39"]
["","","High","dBA","40","43.0","44"]
["Standard Accessories","Installation and operation manual","","","1","1","1"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Sealing pad","","","Sealing pad","Sealing pad","Sealing pad"]
["","Clamps","","","Clamps","Clamps","Clamps"]
["","Screws","","","Screws","Screws","Screws"]
["","Washer","","","Washer","Washer","Washer"]
["","Joint","","","Joint","Joint","Joint"]
["","Holding plate","","","Holding plate","Holding plate","Holding plate"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52"]
["","Gas","OD","mm","15.90","15.90","15.90"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Sound power level","Cooling","","dBA","56","59.0","60"]
["","Heating","","dBA","56","59.0","60"]
["Dimensions","Unit","Width","mm","895","895","895"]
["","","Depth","mm","895","895","895"]
["","","Height","mm","165","230","230"]
["Casing","Material","","","Resin","Resin","Resin"]
["","Colour","","","White","White","White"]
["Weight","Unit","","kg","25.0","31.0","31.0"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","V1","V1","V1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240"]